(footprint "SW_APEM_P36S103"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Body 7.4x7.4mm SMT Hexadecimal Rotary Switches, APEM P36S Series")
	(property "Reference" "REF**"
		(at 0 -4.75 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_APEM_P36S103"
		(at 0 4.675 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(fp_text user "0"
		(at -0.4 -2.053 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "0"
		(at -0.4 -2.053 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -3.75 -2.54 180)
		(size 3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 3.75 2.54 180)
		(size 3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -3.75 2.54 180)
		(size 3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 3.75 -2.54 180)
		(size 3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd rect
		(at -3.75 0 180)
		(size 3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd rect
		(at 3.75 0 180)
		(size 3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
