(footprint "SW_APEM_P60A701"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Body 10x10mm BCD Rotary Switches With Cross shaped slot, APEM P60A Series")
	(property "Reference" "REF**"
		(at 0.00005 -5.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_APEM_P60A701"
		(at 0.00005 5.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "7"
		(at -1.917795 1.064755 108)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "6"
		(at -0.930636 1.985075 144)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at 1.022846 -1.918155 324)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "0"
		(at -0.31995 -2.1775 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "2"
		(at 1.911465 -1.084545 288)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "3"
		(at 2.185145 0.242235 252)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "8"
		(at -2.177365 -0.265875 72)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "9"
		(at -1.621586 -1.483075 36)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "4"
		(at 1.653876 1.459675 216)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "2"
		(at 1.911465 -1.084545 288)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "7"
		(at -1.917795 1.064755 108)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "9"
		(at -1.621586 -1.483075 36)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "0"
		(at -0.4 -2.153 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "3"
		(at 2.185145 0.242235 252)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "8"
		(at -2.177365 -0.265875 72)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "6"
		(at -0.930636 1.985075 144)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "4"
		(at 1.653876 1.459675 216)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "1"
		(at 1.022846 -1.918155 324)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "5"
		(at 0.4449 2.153 180)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at -3.80995 -3.81 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at -1.26995 -3.81 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at 1.27005 -3.81 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "8" thru_hole circle
		(at 3.81005 -3.81 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "C" thru_hole circle
		(at -1.26995 3.81)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
