(footprint "SW_APEM_PT65103"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Body 10x10mm, Straight Rotary Hexadecimal Code Switch Whith Screwdriver Actuator, APEM PT65 (CR65) Series")
	(property "Reference" "REF**"
		(at 0.00004 -5.80001 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_APEM_PT65103"
		(at 0.00004 5.80001 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "0"
		(at -0.39991 -2.753 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "D"
		(at -2.69647 -0.683976 67.5)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "B"
		(at -2.39033 1.423076 112.5)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "5"
		(at 2.69656 0.683976 247.5)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "8"
		(at 0.40005 2.753 180)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "6"
		(at 2.209355 1.684025 225)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "E"
		(at -2.209265 -1.684025 45)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "7"
		(at 1.423126 2.39037 202.5)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "0"
		(at -0.39996 -2.753 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "C"
		(at -2.75296 0.42857 90)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "9"
		(at -0.710326 2.68558 157.5)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "4"
		(at 2.75305 -0.42857 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "3"
		(at 2.39042 -1.423086 292.5)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "A"
		(at -1.623375 2.269915 135)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "2"
		(at 1.663865 -2.229515 315)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "F"
		(at -1.396636 -2.40131 22.5)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "1"
		(at 0.921586 -2.59811 337.5)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at -3.81 -2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at 3.81 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at -3.81 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "8" thru_hole circle
		(at 3.81 -2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "C1" thru_hole circle
		(at -3.81 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "C2" thru_hole circle
		(at 3.81 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
