(footprint "SW_APEM_PT65121"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Body 10x10mm, Decimal Code 4 Positions Straight Rotary Switch Whith Arrow Shaped Slot Actuator, APEM PT65 (CR65) Series")
	(property "Reference" "REF**"
		(at 0 -5.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_APEM_PT65121"
		(at 0 5.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "2"
		(at 0.4 2.753 180)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "0"
		(at -0.4 -2.753 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "2"
		(at 0.4 2.753 180)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "1"
		(at 2.753 -0.42857 270)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "3"
		(at -2.753 0.42857 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "0"
		(at -0.4 -2.753 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at -3.81 -2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at 3.81 -2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at 3.81 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at -3.81 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "C1" thru_hole circle
		(at -3.81 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "C2" thru_hole circle
		(at 3.81 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
