(footprint "SW_C&K_1101M2S3AV2BE2"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Vertical Right Angled PC Thru-Hole SPDT Slide Switch, .200\" High Actuator, C&K 1000 Series")
	(property "Reference" "REF**"
		(at -7.31386 -4.102 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_C&K_1101M2S3AV2BE2"
		(at -7.31386 4.102 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(pad "1" thru_hole circle
		(at -3.80996 0 270)
		(size 2.5 2.5)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at 0.00004 0 270)
		(size 2.5 2.5)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at 3.81005 0 270)
		(size 2.5 2.5)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at -13.96996 -2.225)
		(size 2.3 2.3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at -13.96996 2.225)
		(size 2.3 2.3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
