(footprint "SW_C&K_7101J1AQE2"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Right Angled PC Thru-Hole SPDT Rocker Switch, .531\" Long Horizontal Actuator, C&K 7000 Series")
	(property "Reference" "REF**"
		(at -12.40097 -9.06823 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_C&K_7101J1AQE2"
		(at -12.40097 9.02716 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "3"
		(at -3.87742 -5.18929 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "2"
		(at -4.67742 0.40734 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -4.17742 5.69 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "3"
		(at -3.87742 -5.18929 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "2"
		(at -4.67742 0.40734 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "1"
		(at -4.17742 5.69 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(pad "" smd custom
		(at -13.1532 4)
		(size 0.000001 0.000001)
		(layers "F.Cu")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0 0) (xy 0 2.38696) (xy 0.9064 2.38696) (xy 0.9064 0)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -13.14499 -6.28642)
		(size 0.000001 0.000001)
		(layers "F.Cu")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0 0) (xy 0.88997 0) (xy 0.88995 2.28642) (xy 0 2.28641)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -7.3112 1.77408)
		(size 0.000001 0.000001)
		(layers "F.Cu")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0 0) (xy 0 -3.548) (xy 0.9064 -3.548) (xy 0.9064 0)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 4.7)
		(size 2.5 2.5)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at 0 0)
		(size 2.5 2.5)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at 0 -4.7)
		(size 2.5 2.5)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "P1" thru_hole circle
		(at -12.7 -2.54)
		(size 2.3 2.3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "P1" thru_hole circle
		(at -12.7 2.54)
		(size 2.3 2.3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
