(footprint "SW_C&K_AYZ0202AGRLC"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Body 7.2x3.5mm, DPDT Right Angle Slide Miniature Switch, Surface Mount, AYZ Series")
	(property "Reference" "REF**"
		(at 0 -4.375 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_C&K_AYZ0202AGRLC"
		(at 0 4.375 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "" np_thru_hole circle
		(at -1.5 0)
		(size 0.5 0.5)
		(drill 0.85)
		(layers "F&B.Cu" "*.Mask")
		(solder_mask_margin 0.175)
		(thermal_bridge_angle 90)
	)
	(pad "" np_thru_hole circle
		(at 1.5 0)
		(size 0.5 0.5)
		(drill 0.85)
		(layers "F&B.Cu" "*.Mask")
		(solder_mask_margin 0.175)
		(thermal_bridge_angle 90)
	)
	(pad "1" smd rect
		(at -2.5 -2.825 90)
		(size 1.15 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0 -2.825 90)
		(size 1.15 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 2.5 -2.825 90)
		(size 1.15 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -2.5 2.825 90)
		(size 1.15 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 0 2.825 90)
		(size 1.15 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 2.5 2.825 90)
		(size 1.15 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
