(footprint "SW_C&K_BPA02SB"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Body 7x8.15mm, 2 Ways SPST Surface-Mount DIP Switch, Side Actuator, BPA Series")
	(property "Reference" "REF**"
		(at 0 -6.18 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_C&K_BPA02SB"
		(at 0 7.475 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(fp_text user "1"
		(at -2.8 5.53539 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(pad "1" smd rect
		(at -1.27 4.13)
		(size 1.52 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 1.27 4.13)
		(size 1.52 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 1.27 -4.13)
		(size 1.52 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.27 -4.13)
		(size 1.52 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
