(footprint "SW_C&K_BPA06SB"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Body 17.2x8.15mm, 8 Ways SPST Surface-Mount DIP Switch, Side Actuator, BPA Series")
	(property "Reference" "REF**"
		(at -0.6475 -9.56484 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_C&K_BPA06SB"
		(at -0.6475 9.58516 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(fp_text user "1"
		(at -2.4695 -6.47684 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "6"
		(at -2.4695 6.12317 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "6"
		(at -2.4695 6.12317 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "1"
		(at -2.4695 -6.47684 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -4.13 -6.34984 270)
		(size 1.52 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -4.13 -3.80984 270)
		(size 1.52 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -4.13 -1.26984 270)
		(size 1.52 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -4.13 1.27016 270)
		(size 1.52 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -4.13 3.81016 270)
		(size 1.52 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -4.13 6.35016 270)
		(size 1.52 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 4.13 6.35016 270)
		(size 1.52 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 4.13 3.81016 270)
		(size 1.52 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 4.13 1.27016 270)
		(size 1.52 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 4.13 -1.26984 270)
		(size 1.52 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 4.13 -3.80984 270)
		(size 1.52 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 4.13 -6.34984 270)
		(size 1.52 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
