(footprint "SW_C&K_PCM13SMTR"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SP3T, Right Angled Ultraminiature Surface Mount Slide Switches, C&K PCM Series")
	(property "Reference" "REF**"
		(at 0 -3.475 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_C&K_PCM13SMTR"
		(at 0 3.775 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "" np_thru_hole circle
		(at -2.5 0)
		(size 0.5 0.5)
		(drill 0.9)
		(layers "F&B.Cu" "*.Mask")
		(solder_mask_margin 0.2)
		(thermal_bridge_angle 90)
	)
	(pad "" np_thru_hole circle
		(at 2.5 0)
		(size 0.5 0.5)
		(drill 0.9)
		(layers "F&B.Cu" "*.Mask")
		(solder_mask_margin 0.2)
		(thermal_bridge_angle 90)
	)
	(pad "1" smd rect
		(at -3 -1.75)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.5 -1.75)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 1.5 -1.75367)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 3 -1.75)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -5.15 -0.965)
		(size 1 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -5.15 0.965)
		(size 1 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 5.15 -0.965)
		(size 1 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 5.15 0.965)
		(size 1 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
