(footprint "SW_CTS_204-124ST"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Body 22.5 x 9.78mm 4 x SPDT DIP Switch, 204 Series")
	(property "Reference" "REF**"
		(at -0.29 -12.225 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_CTS_204-124ST"
		(at -0.29 12.225 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(fp_text user "1"
		(at -5.86 -9.9965 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -5.859 -10.0015 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -4.3 -8.89 270)
		(size 1.13 2.44)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -4.3 -6.35 270)
		(size 1.13 2.44)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -4.3 -3.81 270)
		(size 1.13 2.44)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -4.3 -1.27 270)
		(size 1.13 2.44)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -4.3 1.27 270)
		(size 1.13 2.44)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -4.3 3.81 270)
		(size 1.13 2.44)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -4.3 6.35 270)
		(size 1.13 2.44)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -4.3 8.89 270)
		(size 1.13 2.44)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 4.3 8.89 270)
		(size 1.13 2.44)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 4.3 6.35 270)
		(size 1.13 2.44)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 4.3 3.81 270)
		(size 1.13 2.44)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 4.3 1.27 270)
		(size 1.13 2.44)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 4.3 -1.27 270)
		(size 1.13 2.44)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 4.3 -3.81 270)
		(size 1.13 2.44)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 4.3 -6.35 270)
		(size 1.13 2.44)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 4.3 -8.89 270)
		(size 1.13 2.44)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
