(footprint "SW_CTS_206-125"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Body 27.3 x 9.7mm 5 SPDT DIP Slide Switch, SPST DIP Switch, CTS 206 Series")
	(property "Reference" "REF**"
		(at -0.375 -14.775 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_CTS_206-125"
		(at -0.375 14.775 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(fp_text user "1"
		(at -5.36 -14.3765 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -5.359 -14.3815 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at -3.81 -11.43 270)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at -3.81 -8.89 270)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at -3.81 -6.35 180)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at -3.81 -3.81 180)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at -3.81 -1.27 270)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6" thru_hole circle
		(at -3.81 1.27 270)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "7" thru_hole circle
		(at -3.81 3.81 180)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "8" thru_hole circle
		(at -3.81 6.35 180)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "9" thru_hole circle
		(at -3.81 8.89 180)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "10" thru_hole circle
		(at -3.81 11.43 180)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "11" thru_hole circle
		(at 3.81 11.43 180)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "12" thru_hole circle
		(at 3.81 8.89 180)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "13" thru_hole circle
		(at 3.81 6.35 180)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "14" thru_hole circle
		(at 3.81 3.81 180)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "15" thru_hole circle
		(at 3.81 1.27 180)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "16" thru_hole circle
		(at 3.81 -1.27 180)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "17" thru_hole circle
		(at 3.81 -3.81 180)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "18" thru_hole circle
		(at 3.81 -6.35 180)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "19" thru_hole circle
		(at 3.81 -8.89 180)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "20" thru_hole circle
		(at 3.81 -11.43 180)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
