(footprint "SW_DIPTRONICS_DHA-04TQ"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Pitch 1.27mm,  Body 6.2x6.21mm, 4 Ways SPST Surface-Mount DIP Switch, DIPTRONICS DHA Series")
	(property "Reference" "REF**"
		(at 0 -4.074 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_DIPTRONICS_DHA-04TQ"
		(at 0 4.076 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(fp_text user "ON"
		(at 1.2725 -2.54 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "3"
		(at -2.5035 0.38 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "4"
		(at -2.5035 1.65 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "2"
		(at -2.5035 -0.89 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -2.5035 -2.16 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "ON"
		(at 1.2825 -2.54 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "4"
		(at -2.4985 1.651 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "2"
		(at -2.4985 -0.889 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "1"
		(at -2.4985 -2.159 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "3"
		(at -2.4985 0.381 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -3.81 -1.905)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -3.81 -0.635)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -3.81 0.635)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -3.81 1.905)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 3.81 1.905)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 3.81 0.635)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 3.81 -0.635)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 3.81 -1.905)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
