(footprint "SW_DIPTRONICS_DHA-08TQ"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Pitch 1.27mm,  Body 6.2x11.29mm, 8 Ways SPST Surface-Mount DIP Switch, DIPTRONICS DHA Series")
	(property "Reference" "REF**"
		(at 0 -6.62 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_DIPTRONICS_DHA-08TQ"
		(at 0 6.62 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(fp_text user "5"
		(at -2.4085 0.381 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "2"
		(at -2.4085 -3.429 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "8"
		(at -2.4085 4.191 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "6"
		(at -2.4085 1.651 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "7"
		(at -2.4085 2.921 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "3"
		(at -2.4085 -2.159 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "4"
		(at -2.4085 -0.889 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -2.4085 -4.699 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "ON"
		(at 1.1475 -5.08 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "7"
		(at -2.3985 2.921 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "6"
		(at -2.3985 1.651 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "8"
		(at -2.3985 4.191 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "4"
		(at -2.3985 -0.889 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "3"
		(at -2.3985 -2.159 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "5"
		(at -2.3985 0.381 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "2"
		(at -2.3985 -3.429 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "ON"
		(at 1.1575 -5.08 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "1"
		(at -2.3985 -4.699 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -3.81 -4.441)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -3.81 -3.171)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -3.81 -1.901)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -3.81 -0.631)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -3.81 0.639)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -3.81 1.909)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -3.81 3.179)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -3.81 4.449)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 3.81 4.449)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 3.81 3.179)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 3.81 1.909)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 3.81 0.639)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 3.81 -0.631)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 3.81 -1.901)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 3.81 -3.171)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 3.81 -4.441)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
