(footprint "SW_E-SWITCH_1004P3T2B4M7QE"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Pitch 4.7mm, Body 21.59x12.7mm, Vertical 4PDT Toggle Switch ON-OFF-ON, Contact Rating 20V 0.4VAC, Contact Gold, 100 Series")
	(property "Reference" "REF**"
		(at -0.000001 -12.985 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_E-SWITCH_1004P3T2B4M7QE"
		(at -0.000001 25.57 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(pad "1" thru_hole circle
		(at -7.245 -3.365 180)
		(size 2.6 2.6)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at -7.245 -7.175 180)
		(size 2.6 2.6)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at -7.245 -10.985 180)
		(size 2.6 2.6)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at -2.415 -3.365 180)
		(size 2.6 2.6)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at -2.415 -7.175 180)
		(size 2.6 2.6)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6" thru_hole circle
		(at -2.415 -10.985 180)
		(size 2.6 2.6)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "7" thru_hole circle
		(at 2.415 -3.365 180)
		(size 2.6 2.6)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "8" thru_hole circle
		(at 2.415 -7.175 180)
		(size 2.6 2.6)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "9" thru_hole circle
		(at 2.415 -10.985 180)
		(size 2.6 2.6)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "10" thru_hole circle
		(at 7.245 -3.365 180)
		(size 2.6 2.6)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "11" thru_hole circle
		(at 7.245 -7.175 180)
		(size 2.6 2.6)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "12" thru_hole circle
		(at 7.245 -10.985 180)
		(size 2.6 2.6)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "MECH1" thru_hole circle
		(at -2.54 10.985 180)
		(size 2.6 2.6)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "MECH2" thru_hole circle
		(at 2.54 10.985 180)
		(size 2.6 2.6)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
