(footprint "SW_E-SWITCH_100SP1T1B3M2QEH"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Pitch 4.7mm, Body 12.7x6.86mm, Vertical SPDT Toggle Switch ON-OFF-ON, Contact Rating 2A 250VAC, 100 Serie")
	(property "Reference" "REF**"
		(at -0.002395 -7.15239 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_E-SWITCH_100SP1T1B3M2QEH"
		(at -0.002395 7.14761 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(pad "1" thru_hole circle
		(at 0 -4.7 180)
		(size 2.6 2.6)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at 0 0 180)
		(size 2.6 2.6)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at 0 4.7 180)
		(size 2.6 2.6)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
