(footprint "SW_E-SWITCH_EGL2290R"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Surface Mount DP2T Illuminated Slide Switch (Red LED Version), Body 7.65 x 5.5mm")
	(property "Reference" "REF**"
		(at 0 -5.975 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_E-SWITCH_EGL2290R"
		(at 0 5.975 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(fp_text user "3"
		(at 3.358 4.8395 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "4"
		(at -4.042 -3.5605 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at 3.433 -3.6105 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "6"
		(at -3.992 4.8645 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "3"
		(at 3.358 4.8395 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "4"
		(at -4.042 -3.5605 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "6"
		(at -3.992 4.8645 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "1"
		(at 3.433 -3.6105 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at 3.25 -2.5)
		(size 1.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 3.25 0)
		(size 1.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 3.25 2.5)
		(size 1.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -3.25 -2.5)
		(size 1.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -3.25 0)
		(size 1.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -3.25 2.5)
		(size 1.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 0 -4.25 90)
		(size 1.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 0 4.25 90)
		(size 1.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
