(footprint "SW_E-SWITCH_TL3315NF100Q"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Tactile Switch SPST-NO Top Actuated Surface Mount, 0.05A @ 15V")
	(property "Reference" "REF**"
		(at 0 -3.225 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_E-SWITCH_TL3315NF100Q"
		(at 0 3.225 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -2.47522 -1.75)
		(size 0.2 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd rect
		(at -2.14722 -1.75)
		(size 0.5 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 2.14722 -1.75 180)
		(size 0.5 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 2.47522 -1.75 180)
		(size 0.2 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -2.47522 1.75)
		(size 0.2 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -2.14722 1.75)
		(size 0.5 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 2.14722 1.75 180)
		(size 0.5 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 2.47522 1.75 180)
		(size 0.2 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
