(footprint "SW_ERG_DS16C1-8"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "PackageDescription  Body 22.7x9.9mm, Pitch 2.54mm, 1 Pole 8 Ways (SP8T), Thru Hole DIP Switch, ERG DS16C Serie")
	(property "Reference" "REF**"
		(at 0 -11.80001 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_ERG_DS16C1-8"
		(at 0 12.50001 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "3"
		(at -2.9895 -4.191 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "5"
		(at -2.9895 0.889 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "6"
		(at -2.9895 3.429 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "7"
		(at -2.9895 5.969 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "2"
		(at -2.9895 -6.731 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "4"
		(at -2.9895 -1.651 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "8"
		(at -2.9895 8.509 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -2.9895 -9.017 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "6"
		(at -2.9895 3.429 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "4"
		(at -2.9895 -1.651 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "7"
		(at -2.9895 5.969 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "1"
		(at -2.9895 -9.017 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "3"
		(at -2.9895 -4.191 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "5"
		(at -2.9895 0.889 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "2"
		(at -2.9895 -6.731 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "8"
		(at -2.9895 8.509 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at -3.81 -8.89 270)
		(size 1.3 1.3)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at -3.81 -6.35 270)
		(size 1.3 1.3)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at -3.81 -3.81 270)
		(size 1.3 1.3)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at -3.81 -1.27 270)
		(size 1.3 1.3)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at -3.81 1.27 270)
		(size 1.3 1.3)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6" thru_hole circle
		(at -3.81 3.81 270)
		(size 1.3 1.3)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "7" thru_hole circle
		(at -3.81 6.35 270)
		(size 1.3 1.3)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "8" thru_hole circle
		(at -3.81 8.89 270)
		(size 1.3 1.3)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "9" thru_hole circle
		(at 3.81 8.89 270)
		(size 1.3 1.3)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "10" thru_hole circle
		(at 3.81 6.35 270)
		(size 1.3 1.3)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "11" thru_hole circle
		(at 3.81 3.81 270)
		(size 1.3 1.3)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "12" thru_hole circle
		(at 3.81 1.27 270)
		(size 1.3 1.3)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "13" thru_hole circle
		(at 3.81 -1.27 270)
		(size 1.3 1.3)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "14" thru_hole circle
		(at 3.81 -3.81 270)
		(size 1.3 1.3)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "15" thru_hole circle
		(at 3.81 -6.35 270)
		(size 1.3 1.3)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "16" thru_hole circle
		(at 3.81 -8.89 270)
		(size 1.3 1.3)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
