(footprint "SW_LORLIN_CK_3-POLES"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "3 Pole 4 Ways, Rotary Switch, LORLIN CK Serie")
	(property "Reference" "REF**"
		(at 0 -13.90001 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_LORLIN_CK_3-POLES"
		(at 0 13.90001 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "A"
		(at -1.034432 0.97774 120)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "4"
		(at -5.605171 -1.030312 75)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "B"
		(at -0.32953 -1.38471 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "C"
		(at 1.363962 0.40697 240)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "11"
		(at 4.465364 3.541173 227)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "8"
		(at 3.658249 -4.302459 315)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "5"
		(at -4.339059 -3.694859 45)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "12"
		(at 2.188698 5.262033 198)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "3"
		(at -5.369371 1.910312 105)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "7"
		(at 1.016912 -5.555161 345)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "6"
		(at -1.910312 -5.369371 15)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "2"
		(at -3.694859 4.339059 135)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "10"
		(at 5.651405 0.735546 258)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "9"
		(at 5.319371 -1.996912 285)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -1.225317 5.565799 163)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -1.225317 5.565799 163)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "5"
		(at -4.339059 -3.694859 45)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "3"
		(at -5.369371 1.910312 105)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "10"
		(at 5.651405 0.735546 258)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "B"
		(at -0.32953 -1.38471 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "A"
		(at -1.034432 0.97774 120)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "12"
		(at 2.188698 5.262033 198)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "2"
		(at -3.694859 4.339059 135)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "4"
		(at -5.605171 -1.030312 75)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "9"
		(at 5.319371 -1.996912 285)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "6"
		(at -1.910312 -5.369371 15)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "11"
		(at 4.465364 3.541173 227)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "8"
		(at 3.658249 -4.302459 315)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "C"
		(at 1.363962 0.40697 240)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "7"
		(at 1.016912 -5.555161 345)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at -2.84701 10.62519 270)
		(size 2 2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at -7.77818 7.77818 270)
		(size 2 2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at -10.62519 2.84701 270)
		(size 2 2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at -10.62519 -2.84701 270)
		(size 2 2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at -7.77818 -7.77818 270)
		(size 2 2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6" thru_hole circle
		(at -2.84701 -10.62519 270)
		(size 2 2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "7" thru_hole circle
		(at 2.84701 -10.62519 270)
		(size 2 2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "8" thru_hole circle
		(at 7.77818 -7.77818 270)
		(size 2 2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "9" thru_hole circle
		(at 10.62519 -2.84701 270)
		(size 2 2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "10" thru_hole circle
		(at 10.62519 2.84701 270)
		(size 2 2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "11" thru_hole circle
		(at 7.77818 7.77818 270)
		(size 2 2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "12" thru_hole circle
		(at 2.84701 10.62519 270)
		(size 2 2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "A" thru_hole circle
		(at -3.3342 1.925 225)
		(size 2 2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "B" thru_hole circle
		(at 0 -3.85 225)
		(size 2 2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "C" thru_hole circle
		(at 3.3342 1.925 225)
		(size 2 2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
