(footprint "SW_MULTICOMP_4US1R202M2RN"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Pitch 2.45mm, Body 7.5x5mm, SPDT Switch, On-On, Lever")
	(property "Reference" "REF**"
		(at 0 -4.55 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_MULTICOMP_4US1R202M2RN"
		(at 0 4.55 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "4"
		(at -0.52 -1.9175 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "5"
		(at -0.52 0.6225 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "6"
		(at -0.52 3.1625 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(pad "1" thru_hole circle
		(at 1.27 -2.54)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at 1.27 2.54)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at -1.27 -2.54)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at -1.27 0)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6" thru_hole circle
		(at -1.27 2.54)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
