(footprint "SW_NIDEC_CVS-03TB"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Body 4.7x4mm, SPDT Slide Switch, Surface Mount, CVS Series")
	(property "Reference" "REF**"
		(at 0 -3.375 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_NIDEC_CVS-03TB"
		(at 0 3.375 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(fp_text user "ON"
		(at 0.95 -2.076995 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(pad "1" smd rect
		(at -2.95 -1)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.95 0)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -2.95 1)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 2.95 1)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 2.95 0)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 2.95 -1)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MECH" smd rect
		(at -2.15 -1.95)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MECH" smd rect
		(at -2.15 1.95)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MECH" smd rect
		(at 2.15 -1.95)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MECH" smd rect
		(at 2.15 1.95)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
