(footprint "SW_NKK_A13AV"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "BBody 5x10.2mm, Vertical Right Angle PCB Mounting, SPDT ON-OFF-ON Switch, NKK A Series")
	(property "Reference" "REF**"
		(at -8.95385 -2.8066 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_NKK_A13AV"
		(at -8.95385 4.6354 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(pad "" smd custom
		(at -11.45556 -1.5494)
		(size 0.000001 0.000001)
		(layers "F.Cu")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0 0) (xy 0.3048 0) (xy 0.3048 0.889) (xy 0 0.889)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -11.45556 2.6416)
		(size 0.000001 0.000001)
		(layers "F.Cu")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0 0) (xy 0.3048 0) (xy 0.3048 0.889) (xy 0 0.889)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -5.23257 3.45)
		(size 0.000001 0.000001)
		(layers "F.Cu")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0 0) (xy 0.3048 0) (xy 0.30481 0.0806) (xy 0.00001 0.0806)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -5.23256 -1.5494)
		(size 0.000001 0.000001)
		(layers "F.Cu")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0 0) (xy 0.3048 0) (xy 0.3048 0.889) (xy 0 0.889)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 2.53984 0 270)
		(size 1.5 1.5)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at -0.00016 0 270)
		(size 1.5 1.5)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at -2.54017 0 270)
		(size 1.5 1.5)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at -7.62017 0)
		(size 1.5 1.5)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at -5.08016 2.54)
		(size 1.5 1.5)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
