(footprint "SW_NKK_UB225SKG035F"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Body 15.24x15.24mm, Straight PCB Mounting Momentary Illuminated Pushbutton, Bright LED, Clear Lens/Green Diffuser , NKK UB2 Series")
	(property "Reference" "REF**"
		(at -0.00051 -8.41978 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_NKK_UB225SKG035F"
		(at -0.00051 8.41776 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "COM"
		(at 3.7 3.62446 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "NC"
		(at -5.9 -2.37554 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "COM"
		(at -6.4 3.62446 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "NO"
		(at -3.7 1.92446 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "L+"
		(at -1.2 -4.21331 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "NO"
		(at 2 1.92446 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "NC"
		(at 4.2 -2.37554 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "L-"
		(at -1.2 5.98669 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(pad "1" thru_hole circle
		(at 5.08 5.08)
		(size 1.9 1.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at 5.08 0)
		(size 1.9 1.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at 5.08 -5.08)
		(size 1.9 1.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at -5.08 5.08)
		(size 1.9 1.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at -5.08 0)
		(size 1.9 1.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6" thru_hole circle
		(at -5.08 -5.08)
		(size 1.9 1.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "7" thru_hole circle
		(at 0 2.54)
		(size 1.9 1.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "8" thru_hole circle
		(at 0 -2.54)
		(size 1.9 1.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
