(footprint "SW_OMRON_A6H-6102"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Pitch 1.27mm, Body 8.85 x 4.5mm, 6 Ways SPST Surface-Mounting DIP Switch, OMRON A6H")
	(property "Reference" "REF**"
		(at 0 -5.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_OMRON_A6H-6102"
		(at 0 5.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(fp_text user "1"
		(at -3.8055 -4.445 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(pad "1" smd rect
		(at -3.075 -3.175)
		(size 1.25 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -3.075 -1.905)
		(size 1.25 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -3.075 -0.635)
		(size 1.25 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -3.075 0.635)
		(size 1.25 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -3.075 1.905)
		(size 1.25 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -3.075 3.175)
		(size 1.25 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 3.075 3.175)
		(size 1.25 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 3.075 1.905)
		(size 1.25 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 3.075 0.635)
		(size 1.25 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 3.075 -0.635)
		(size 1.25 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 3.075 -1.905)
		(size 1.25 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 3.075 -3.175)
		(size 1.25 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
