(footprint "SW_OMRON_A6SN-8101"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Pitch 2.54mm, Body 22.3x7.5, 8 Ways SPST Surface-Mounting Slide Switch With Flat Actuator (A6SN Series)")
	(property "Reference" "REF**"
		(at 0 -12.355 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_OMRON_A6SN-8101"
		(at 0 12.355 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(fp_text user "8"
		(at -3.2975 10.31875 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "ON"
		(at 1.8778 -10.008937 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -3.2975 -10.795 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(pad "1" smd rect
		(at -4.125 -8.89)
		(size 2.15 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -4.125 -6.35)
		(size 2.15 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -4.125 -3.81)
		(size 2.15 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -4.125 -1.27)
		(size 2.15 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -4.125 1.27)
		(size 2.15 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -4.125 3.81)
		(size 2.15 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -4.125 6.35)
		(size 2.15 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -4.125 8.89)
		(size 2.15 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 4.125 8.89)
		(size 2.15 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 4.125 6.35)
		(size 2.15 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 4.125 3.81)
		(size 2.15 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 4.125 1.27)
		(size 2.15 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 4.125 -1.27)
		(size 2.15 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 4.125 -3.81)
		(size 2.15 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 4.125 -6.35)
		(size 2.15 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 4.125 -8.89)
		(size 2.15 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
