(footprint "SW_RS_734-7270"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Body 11.43x12.7mm, DPDT Vertical Slide Subminiature Switch, Thru-Hole Mount")
	(property "Reference" "REF**"
		(at 0 -7.15 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_RS_734-7270"
		(at 0 7.15 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "1"
		(at -6.2 -4.66461 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(pad "1" thru_hole circle
		(at -2.415 -4.7)
		(size 2.55 2.55)
		(drill 1.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at -2.415 0)
		(size 2.55 2.55)
		(drill 1.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at -2.415 4.7)
		(size 2.55 2.55)
		(drill 1.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at 2.415 -4.7)
		(size 2.55 2.55)
		(drill 1.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at 2.415 0)
		(size 2.55 2.55)
		(drill 1.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6" thru_hole circle
		(at 2.415 4.7)
		(size 2.55 2.55)
		(drill 1.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
