(footprint "SW_TYCO_1571983-8"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Pitch 1.27mm,  Body 6.2x8.74mm, 6 Ways SPST Surface-Mount DIP Switch, TYCO GDH Serie")
	(property "Reference" "REF**"
		(at 0 -5.345 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_TYCO_1571983-8"
		(at 0 5.345 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(fp_text user "2"
		(at -2.4225 -2.2 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "5"
		(at -2.4225 1.61 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "ON"
		(at 1.1775 -3.8 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -2.4225 -3.4 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "6"
		(at -2.4225 2.88 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "3"
		(at -2.4225 -1 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "4"
		(at -2.4225 0.34 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "4"
		(at -2.4225 0.34 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "3"
		(at -2.4225 -1 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "2"
		(at -2.4225 -2.2 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "6"
		(at -2.4225 2.88 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "5"
		(at -2.4225 1.61 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "1"
		(at -2.4225 -3.4 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "ON"
		(at 1.1775 -3.8 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -3.795 -3.175)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -3.795 -1.905)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -3.795 -0.635)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -3.795 0.635)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -3.795 1.905)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -3.795 3.175)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 3.795 3.175)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 3.795 1.905)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 3.795 0.635)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 3.795 -0.635)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 3.795 -1.905)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 3.795 -3.175)
		(size 1.27 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
