(footprint "SW_TYCO_1825010-5"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Pitch 2.54mm,  Body 10.16x7.36mm, SMD DPDT Slide DIP Switch, Extented Top Actuator, TYCO ASE/F Series")
	(property "Reference" "REF**"
		(at 0.000045 -6.055 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_TYCO_1825010-5"
		(at 0.000045 6.055 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -4.12746 -2.54)
		(size 2.159 1.02)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -4.12746 0)
		(size 2.159 1.02)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -4.12746 2.54)
		(size 2.159 1.02)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 4.12755 2.54)
		(size 2.159 1.02)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 4.12755 0)
		(size 2.159 1.02)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 4.12755 -2.54)
		(size 2.159 1.02)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
