(footprint "SW_TYCO_1825057-1"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Body 7.1x7.5mm, 2 Ways SPST DIP Switch, Thru Hole, TYCO AD Series")
	(property "Reference" "REF**"
		(at 0 -4.3306 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_TYCO_1825057-1"
		(at 0 4.3306 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "2"
		(at -2.7895 0.889 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "ON"
		(at 1.5775 -2.1 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -2.7895 -1.397 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "ON"
		(at 1.5775 -2.1 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "1"
		(at -2.7895 -1.397 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "2"
		(at -2.7895 0.889 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at -3.81 -1.27 270)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at -3.81 1.27 270)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at 3.81 1.27 270)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at 3.81 -1.27 270)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
