(footprint "SW_TYCO_1825057-7"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Body 22.3x7.5mm, 8 Ways SPST DIP Switch, Thru Hole, TYCO AD Series")
	(property "Reference" "REF**"
		(at 0 -11.9506 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_TYCO_1825057-7"
		(at 0 11.9506 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "ON"
		(at 1.6555 -9.779 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "2"
		(at -2.7895 -6.731 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "4"
		(at -2.7895 -1.651 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -2.7895 -9.017 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "6"
		(at -2.7895 3.429 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "7"
		(at -2.7895 5.969 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "5"
		(at -2.7895 0.889 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "8"
		(at -2.7895 8.509 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "3"
		(at -2.7895 -4.191 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "6"
		(at -2.7895 3.429 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "7"
		(at -2.7895 5.969 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "4"
		(at -2.7895 -1.651 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "ON"
		(at 1.6555 -9.779 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "3"
		(at -2.7895 -4.191 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "1"
		(at -2.7895 -9.017 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "5"
		(at -2.7895 0.889 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "2"
		(at -2.7895 -6.731 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "8"
		(at -2.7895 8.509 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at -3.81 -8.89 270)
		(size 1.4 1.4)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at -3.81 -6.35 270)
		(size 1.4 1.4)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at -3.81 -3.81 270)
		(size 1.4 1.4)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at -3.81 -1.27 270)
		(size 1.4 1.4)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at -3.81 1.27 270)
		(size 1.4 1.4)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6" thru_hole circle
		(at -3.81 3.81 270)
		(size 1.4 1.4)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "7" thru_hole circle
		(at -3.81 6.35 270)
		(size 1.4 1.4)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "8" thru_hole circle
		(at -3.81 8.89 270)
		(size 1.4 1.4)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "9" thru_hole circle
		(at 3.81 8.89 270)
		(size 1.4 1.4)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "10" thru_hole circle
		(at 3.81 6.35 270)
		(size 1.4 1.4)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "11" thru_hole circle
		(at 3.81 3.81 270)
		(size 1.4 1.4)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "12" thru_hole circle
		(at 3.81 1.27 270)
		(size 1.4 1.4)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "13" thru_hole circle
		(at 3.81 -1.27 270)
		(size 1.4 1.4)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "14" thru_hole circle
		(at 3.81 -3.81 270)
		(size 1.4 1.4)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "15" thru_hole circle
		(at 3.81 -6.35 270)
		(size 1.4 1.4)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "16" thru_hole circle
		(at 3.81 -8.89 270)
		(size 1.4 1.4)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
