(footprint "SW_TYCO_1825138-5"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DPDT Toggle Switch, Double Pole, Contact Rating 0.4VA 20V, Gemini A Series")
	(property "Reference" "REF**"
		(at 0 -9.874 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_TYCO_1825138-5"
		(at 0 9.874 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "1"
		(at 4.616 5.2845 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "4"
		(at -3.675 7.4725 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "1"
		(at 4.616 5.2745 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "3"
		(at 2.975 -5.9775 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "6"
		(at -3.675 -6.0025 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 2.413 4.699)
		(size 2.6 2.6)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at 2.413 0)
		(size 2.6 2.6)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at 2.413 -4.699)
		(size 2.6 2.6)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at -2.413 4.699)
		(size 2.6 2.6)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at -2.413 0)
		(size 2.6 2.6)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6" thru_hole circle
		(at -2.413 -4.699)
		(size 2.6 2.6)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "7" thru_hole circle
		(at -1.5875 -7.874)
		(size 2.6 2.6)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "8" thru_hole circle
		(at 1.5875 -7.874)
		(size 2.6 2.6)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "9" thru_hole circle
		(at -1.5875 7.874)
		(size 2.6 2.6)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "10" thru_hole circle
		(at 1.5875 7.874)
		(size 2.6 2.6)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
