(footprint "Trans_WE_10GB-749052051"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Footprint based on: https://www.we-online.com/components/products/datasheet/749052051.pdf")
	(property "Reference" "REF**"
		(at 0 -9.74 0)
		(layer "F.SilkS")
	)
	(property "Value" "Trans_WE_10GB-749052051"
		(at -8.7 11.7 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0.005 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0.005 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -8.7 13 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -8.7 14.2 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -8.7 15.4 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -7.24 -6.98 270)
		(size 0.76 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0)
	)
	(pad "2" smd rect
		(at -7.24 -5.71 270)
		(size 0.76 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0)
	)
	(pad "3" smd rect
		(at -7.24 -4.44 270)
		(size 0.76 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0)
	)
	(pad "4" smd rect
		(at -7.24 -3.17 270)
		(size 0.76 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0)
	)
	(pad "5" smd rect
		(at -7.24 -1.9 270)
		(size 0.76 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0)
	)
	(pad "6" smd rect
		(at -7.24 -0.63 270)
		(size 0.76 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0)
	)
	(pad "7" smd rect
		(at -7.24 0.64 270)
		(size 0.76 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0)
	)
	(pad "8" smd rect
		(at -7.24 1.91 270)
		(size 0.76 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0)
	)
	(pad "9" smd rect
		(at -7.24 3.18 270)
		(size 0.76 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0)
	)
	(pad "10" smd rect
		(at -7.24 4.45 270)
		(size 0.76 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0)
	)
	(pad "11" smd rect
		(at -7.24 5.72 270)
		(size 0.76 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0)
	)
	(pad "12" smd rect
		(at -7.24 6.99 270)
		(size 0.76 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0)
	)
	(pad "13" smd rect
		(at 7.24 6.99 270)
		(size 0.76 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0)
	)
	(pad "14" smd rect
		(at 7.24 5.72 270)
		(size 0.76 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0)
	)
	(pad "15" smd rect
		(at 7.24 4.45 270)
		(size 0.76 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0)
	)
	(pad "16" smd rect
		(at 7.24 3.18 270)
		(size 0.76 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0)
	)
	(pad "17" smd rect
		(at 7.24 1.91 270)
		(size 0.76 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0)
	)
	(pad "18" smd rect
		(at 7.24 0.64 270)
		(size 0.76 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0)
	)
	(pad "19" smd rect
		(at 7.24 -0.63 270)
		(size 0.76 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0)
	)
	(pad "20" smd rect
		(at 7.24 -1.9 270)
		(size 0.76 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0)
	)
	(pad "21" smd rect
		(at 7.24 -3.17 270)
		(size 0.76 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0)
	)
	(pad "22" smd rect
		(at 7.24 -4.44 270)
		(size 0.76 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0)
	)
	(pad "23" smd rect
		(at 7.24 -5.71 270)
		(size 0.76 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0)
	)
	(pad "24" smd rect
		(at 7.24 -6.98 270)
		(size 0.76 2.29)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0)
	)
	(embedded_fonts no)
	(model "antmicro_749052051.glb"
		(offset
			(xyz -0 -0.005 0.25)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 90)
		)
	)
)
