(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "749052051"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "T"
				(at 43.18 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "749052051"
				(at 43.18 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "749052051"
				(at 43.18 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.we-online.com/components/products/datasheet/749052051.pdf"
				(at 43.18 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Pulse Transformers WE-LAN 10GBsT PoE+ 120uH 1Port 1500Vrms"
				(at 43.18 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Würth Elektronik"
				(at 43.18 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "749052051"
				(at 43.18 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 43.18 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 43.18 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, ETHERNET, TRANSFORMER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "749052051_1_1"
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "TD1")
					(number "1")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 2.54)
					(name "D1+")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "D1-")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 2.54)
					(name "TD2")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 2.54)
					(name "D2+")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 2.54)
					(name "D2-")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "TD3")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "D3+")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "D3-")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 2.54)
					(name "TD4")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 2.54)
					(name "D4+")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 2.54)
					(name "D4-")
					(number "12")
				)
				(pin bidirectional line
					(at 29.21 -52.07 180)
					(length 2.54)
					(name "X4-")
					(number "13")
				)
				(pin bidirectional line
					(at 29.21 -41.91 180)
					(length 2.54)
					(name "X4+")
					(number "14")
				)
				(pin bidirectional line
					(at 29.21 -46.99 180)
					(length 2.54)
					(name "TX4")
					(number "15")
				)
				(pin bidirectional line
					(at 29.21 -38.1 180)
					(length 2.54)
					(name "X3-")
					(number "16")
				)
				(pin bidirectional line
					(at 29.21 -27.94 180)
					(length 2.54)
					(name "X3+")
					(number "17")
				)
				(pin bidirectional line
					(at 29.21 -33.02 180)
					(length 2.54)
					(name "TX3")
					(number "18")
				)
				(pin bidirectional line
					(at 29.21 -24.13 180)
					(length 2.54)
					(name "X2-")
					(number "19")
				)
				(pin bidirectional line
					(at 29.21 -13.97 180)
					(length 2.54)
					(name "X2+")
					(number "20")
				)
				(pin bidirectional line
					(at 29.21 -19.05 180)
					(length 2.54)
					(name "TX2")
					(number "21")
				)
				(pin bidirectional line
					(at 29.21 -10.16 180)
					(length 2.54)
					(name "X1-")
					(number "22")
				)
				(pin bidirectional line
					(at 29.21 0 180)
					(length 2.54)
					(name "X1+")
					(number "23")
				)
				(pin bidirectional line
					(at 29.21 -5.08 180)
					(length 2.54)
					(name "TX1")
					(number "24")
				)
			)
			(embedded_fonts no)
		)
)
