(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ALAN-2204"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 58.42 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ALAN-2204"
				(at 58.42 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ALAN-2204"
				(at 58.42 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://abracon.com/Magnetics/lan/ALAN-2204.pdf"
				(at 58.42 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "10/100 Base-T Single Port LAN Transformer w/ PoE+ Extended Temperature"
				(at 58.42 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Abracon"
				(at 58.42 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ALAN-2204"
				(at 58.42 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 58.42 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 58.42 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, ETHERNET, TRANSFORMER"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ALAN-2204_0_0"
				(text "TD+"
					(at 10.16 2.54 0)
				)
				(text "TD-"
					(at 10.16 -2.54 0)
				)
				(text "TX+"
					(at 30.48 2.54 0)
				)
				(text "TX-"
					(at 30.48 -2.54 0)
				)
			)
			(symbol "ALAN-2204_1_1"
				(text "RD+"
					(at 10.16 -10.795 0)
				)
				(text "RD-"
					(at 10.16 -15.875 0)
				)
				(text "TDCT"
					(at 17.145 -8.89 900)
				)
				(text "RDCT"
					(at 17.145 -22.225 900)
				)
				(text "TXCT"
					(at 23.495 -8.89 900)
				)
				(text "RXCT"
					(at 23.495 -22.225 900)
				)
				(text "RX+"
					(at 30.48 -10.795 0)
				)
				(text "RX-"
					(at 30.48 -15.875 0)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "TD+")
					(number "1")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "TDCT")
					(number "2")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "TD-")
					(number "3")
				)
				(pin no_connect line
					(at 41.91 -21.59 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "4")
				)
				(pin no_connect line
					(at 41.91 -21.59 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "5")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "RD+")
					(number "6")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "RDCT")
					(number "7")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "RD-")
					(number "8")
				)
				(pin passive line
					(at 44.45 -10.16 180)
					(length 2.54)
					(name "RX-")
					(number "9")
				)
				(pin passive line
					(at 44.45 -17.78 180)
					(length 2.54)
					(name "RXCT")
					(number "10")
				)
				(pin passive line
					(at 44.45 -7.62 180)
					(length 2.54)
					(name "RX+")
					(number "11")
				)
				(pin no_connect line
					(at 41.91 -21.59 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "12")
				)
				(pin no_connect line
					(at 41.91 -21.59 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "13")
				)
				(pin passive line
					(at 44.45 -2.54 180)
					(length 2.54)
					(name "TX-")
					(number "14")
				)
				(pin passive line
					(at 44.45 -15.24 180)
					(length 2.54)
					(name "TXCT")
					(number "15")
				)
				(pin passive line
					(at 44.45 0 180)
					(length 2.54)
					(name "TX+")
					(number "16")
				)
			)
			(embedded_fonts no)
		)
)
