(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "H1102NLT"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 53.34 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "H1102NLT"
				(at 53.34 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "H1102NLT"
				(at 53.34 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/3/203/1/H1102NL.pdf"
				(at 53.34 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Audio Transformers / Signal Transformers 100Base-T NonPoE 350uH .65Ohms 1-Port"
				(at 53.34 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Pulse Electronics"
				(at 53.34 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "H1102NLT"
				(at 53.34 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 53.34 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 53.34 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, ETHERNET, TRANSFORMER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "H1102NLT_0_0"
				(text "TD+"
					(at 12.065 0.635 0)
				)
				(text "TD-"
					(at 12.065 -6.985 0)
				)
				(text "TX+"
					(at 30.48 0.635 0)
				)
				(text "TX-"
					(at 30.48 -6.985 0)
				)
			)
			(symbol "H1102NLT_1_1"
				(text "RD+"
					(at 12.065 -12.7 0)
				)
				(text "RD-"
					(at 12.065 -20.32 0)
				)
				(text "TDCT0"
					(at 15.875 -8.89 900)
				)
				(text "RDCT0"
					(at 15.875 -22.225 900)
				)
				(text "TXCT0"
					(at 22.225 -8.89 900)
				)
				(text "RXCT0"
					(at 22.225 -22.225 900)
				)
				(text "RX+"
					(at 30.48 -12.7 0)
				)
				(text "RX-"
					(at 30.48 -20.32 0)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "TD0+")
					(number "1")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "TDCT0")
					(number "2")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "TD0-")
					(number "3")
				)
				(pin no_connect line
					(at 41.91 -21.59 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "4")
				)
				(pin no_connect line
					(at 41.91 -21.59 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "5")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "RD0+")
					(number "6")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "RDCT0")
					(number "7")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "RD0-")
					(number "8")
				)
				(pin passive line
					(at 44.45 -10.16 180)
					(length 2.54)
					(name "RX0-")
					(number "9")
				)
				(pin passive line
					(at 44.45 -17.78 180)
					(length 2.54)
					(name "RXCT0")
					(number "10")
				)
				(pin passive line
					(at 44.45 -7.62 180)
					(length 2.54)
					(name "RX0+")
					(number "11")
				)
				(pin no_connect line
					(at 41.91 -21.59 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "12")
				)
				(pin no_connect line
					(at 41.91 -21.59 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "13")
				)
				(pin passive line
					(at 44.45 -2.54 180)
					(length 2.54)
					(name "TX0-")
					(number "14")
				)
				(pin passive line
					(at 44.45 -15.24 180)
					(length 2.54)
					(name "TXCT0")
					(number "15")
				)
				(pin passive line
					(at 44.45 0 180)
					(length 2.54)
					(name "TX0+")
					(number "16")
				)
			)
			(embedded_fonts no)
		)
)
