(footprint "SOIC127P1594X685-24N"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "PS-2473.001-A")
	(tags "Inductor")
	(property "Reference" "L**"
		(at 0.254 -1.27 0)
		(layer "F.SilkS")
	)
	(property "Value" "SOIC127P1594X685-24N"
		(at 0.254 0 0)
		(layer "F.SilkS")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -8.75 11.454 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -8.75 12.653 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -8.75 13.854 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -7.3 -6.986 90)
		(size 0.85 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -7.3 -5.715 90)
		(size 0.85 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -7.3 -4.446 90)
		(size 0.85 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -7.3 -3.176 90)
		(size 0.85 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -7.3 -1.905 90)
		(size 0.85 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -7.3 -0.635 90)
		(size 0.85 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -7.3 0.633 90)
		(size 0.85 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -7.3 1.904 90)
		(size 0.85 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -7.3 3.173 90)
		(size 0.85 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -7.3 4.445 90)
		(size 0.85 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -7.3 5.714 90)
		(size 0.85 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -7.3 6.985 90)
		(size 0.85 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 7.299 6.985 90)
		(size 0.85 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 7.299 5.714 90)
		(size 0.85 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 7.299 4.445 90)
		(size 0.85 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 7.299 3.173 90)
		(size 0.85 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 7.299 1.904 90)
		(size 0.85 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 7.299 0.633 90)
		(size 0.85 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 7.299 -0.635 90)
		(size 0.85 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 7.299 -1.905 90)
		(size 0.85 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 7.299 -3.176 90)
		(size 0.85 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 7.299 -4.446 90)
		(size 0.85 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 7.299 -5.715 90)
		(size 0.85 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 7.299 -6.986 90)
		(size 0.85 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_h6096nl.glb"
		(offset
			(xyz 0 0 1)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 90)
		)
	)
)
