(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "HM5149NL"
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "T"
				(at 41.91 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "HM5149NL"
				(at 41.91 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "HM5149NL"
				(at 41.91 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/447/HM5149NL-3071787.pdf"
				(at 41.91 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Audio Transformers / Signal Transformers 1000BaseT NonPoE 360uH .65Ohms"
				(at 41.91 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "HM5149NL"
				(at 41.91 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Pulse Electronics"
				(at 41.91 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 41.91 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 41.91 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, ETHERNET, TRANSFORMER"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "HM5149NL_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "TD1+")
					(number "1")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "TD1-")
					(number "2")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 2.54)
					(name "TDCT1")
					(number "3")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 2.54)
					(name "TDCT2")
					(number "4")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "TD2+")
					(number "5")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(name "TD2-")
					(number "6")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(name "TD3+")
					(number "7")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 2.54)
					(name "TD3-")
					(number "8")
				)
				(pin passive line
					(at 0 -41.91 0)
					(length 2.54)
					(name "TDCT3")
					(number "9")
				)
				(pin passive line
					(at 0 -59.69 0)
					(length 2.54)
					(name "TDCT4")
					(number "10")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 2.54)
					(name "TD4+")
					(number "11")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 2.54)
					(name "TD4-")
					(number "12")
				)
				(pin passive line
					(at 27.94 -66.04 180)
					(length 2.54)
					(name "TX4-")
					(number "13")
				)
				(pin passive line
					(at 27.94 -53.34 180)
					(length 2.54)
					(name "TX4+")
					(number "14")
				)
				(pin passive line
					(at 27.94 -59.69 180)
					(length 2.54)
					(name "TXCT4")
					(number "15")
				)
				(pin passive line
					(at 27.94 -41.91 180)
					(length 2.54)
					(name "TXCT3")
					(number "16")
				)
				(pin passive line
					(at 27.94 -48.26 180)
					(length 2.54)
					(name "TX3-")
					(number "17")
				)
				(pin passive line
					(at 27.94 -35.56 180)
					(length 2.54)
					(name "TX3+")
					(number "18")
				)
				(pin passive line
					(at 27.94 -30.48 180)
					(length 2.54)
					(name "TX2-")
					(number "19")
				)
				(pin passive line
					(at 27.94 -17.78 180)
					(length 2.54)
					(name "TX2+")
					(number "20")
				)
				(pin passive line
					(at 27.94 -24.13 180)
					(length 2.54)
					(name "TXCT2")
					(number "21")
				)
				(pin passive line
					(at 27.94 -6.35 180)
					(length 2.54)
					(name "TXCT1")
					(number "22")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 2.54)
					(name "TX1-")
					(number "23")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 2.54)
					(name "TX1+")
					(number "24")
				)
			)
			(embedded_fonts no)
		)
)
