(footprint "Trans_PulseElectronics-HX5120NLT"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Audio Transformers / Signal Transformers 1000Base-T NonPoE 350uH .65Ohms 1-Port")
	(tags "Transformer")
	(property "Reference" "REF**"
		(at 0 -8.8 180)
		(layer "F.SilkS")
	)
	(property "Value" "Trans_PulseElectronics-HX5120NLT"
		(at 0 9.75 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -5.75 12.2 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -5.75 13.4 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -5.75 14.6 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -4.51 -6.985 270)
		(size 0.76 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -4.51 -5.715 270)
		(size 0.76 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -4.51 -4.445 270)
		(size 0.76 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -4.51 -3.175 270)
		(size 0.76 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -4.51 -1.905 270)
		(size 0.76 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -4.51 -0.635 270)
		(size 0.76 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -4.51 0.635 270)
		(size 0.76 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -4.51 1.905 270)
		(size 0.76 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -4.51 3.175 270)
		(size 0.76 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -4.51 4.445 270)
		(size 0.76 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -4.51 5.715 270)
		(size 0.76 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -4.51 6.985 270)
		(size 0.76 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 4.51 6.985 270)
		(size 0.76 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 4.51 5.715 270)
		(size 0.76 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at 4.51 4.445 270)
		(size 0.76 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at 4.51 3.175 270)
		(size 0.76 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at 4.51 1.905 270)
		(size 0.76 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 4.51 0.635 270)
		(size 0.76 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 4.51 -0.635 270)
		(size 0.76 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 4.51 -1.905 270)
		(size 0.76 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 4.51 -3.175 270)
		(size 0.76 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at 4.51 -4.445 270)
		(size 0.76 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at 4.51 -5.715 270)
		(size 0.76 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 4.51 -6.985 270)
		(size 0.76 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "antmicro_hx5120nl.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 90)
		)
	)
)
