(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "HX5120NL"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 53.34 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "HX5120NL"
				(at 53.34 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "HX5120NL"
				(at 53.34 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://productfinder.pulseeng.com/doc_type/WEB301/doc_num/HX5120NL/doc_part/HX5120NL.pdf"
				(at 53.34 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Audio Transformers / Signal Transformers 1000Base-T NonPoE 350uH .65Ohms 1-Port"
				(at 53.34 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Pulse Electronics"
				(at 53.34 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "HX5120NL"
				(at 53.34 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 53.34 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 53.34 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, ETHERNET, TRANSFORMER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "HX5120NL_0_0"
				(text "TD+"
					(at 12.7 -10.16 0)
				)
				(text "TD-"
					(at 12.7 -17.78 0)
				)
				(text "TDCT"
					(at 16.51 -19.685 900)
				)
				(text "4X"
					(at 21.59 -8.89 0)
				)
				(text "TXCT"
					(at 22.86 -19.685 900)
				)
				(text "TX+"
					(at 31.115 -10.16 0)
				)
				(text "TX-"
					(at 31.115 -17.78 0)
				)
			)
			(symbol "HX5120NL_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "TD0+")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "TD0-")
					(number "2")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(name "TDCT0")
					(number "3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(name "TDCT1")
					(number "4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "TD1+")
					(number "5")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "TD1-")
					(number "6")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "TD2+")
					(number "7")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "TD2-")
					(number "8")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 2.54)
					(name "TDCT2")
					(number "9")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(name "TDCT3")
					(number "10")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "TD3+")
					(number "11")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "TD3-")
					(number "12")
				)
				(pin passive line
					(at 44.45 -17.78 180)
					(length 2.54)
					(name "TX3-")
					(number "13")
				)
				(pin passive line
					(at 44.45 -15.24 180)
					(length 2.54)
					(name "TX3+")
					(number "14")
				)
				(pin passive line
					(at 44.45 -30.48 180)
					(length 2.54)
					(name "TXCT3")
					(number "15")
				)
				(pin passive line
					(at 44.45 -27.94 180)
					(length 2.54)
					(name "TXCT2")
					(number "16")
				)
				(pin passive line
					(at 44.45 -12.7 180)
					(length 2.54)
					(name "TX2-")
					(number "17")
				)
				(pin passive line
					(at 44.45 -10.16 180)
					(length 2.54)
					(name "TX2+")
					(number "18")
				)
				(pin passive line
					(at 44.45 -7.62 180)
					(length 2.54)
					(name "TX1-")
					(number "19")
				)
				(pin passive line
					(at 44.45 -5.08 180)
					(length 2.54)
					(name "TX1+")
					(number "20")
				)
				(pin passive line
					(at 44.45 -25.4 180)
					(length 2.54)
					(name "TXCT1")
					(number "21")
				)
				(pin passive line
					(at 44.45 -22.86 180)
					(length 2.54)
					(name "TXCT0")
					(number "22")
				)
				(pin passive line
					(at 44.45 -2.54 180)
					(length 2.54)
					(name "TX0-")
					(number "23")
				)
				(pin passive line
					(at 44.45 0 180)
					(length 2.54)
					(name "TX0+")
					(number "24")
				)
			)
			(embedded_fonts no)
		)
)
