(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Trans_TCM2-722X+"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "T"
				(at 38.1 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Trans_TCM2-722X+"
				(at 38.1 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Trans_TCM2-722X+"
				(at 38.1 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.minicircuits.com/pdfs/TCM2-722X+.pdf"
				(at 38.1 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Audio Transformers / Signal Transformers 1:2 CORE & WIRE Transformer, 400-7200 MHz"
				(at 38.1 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TCM2-722X+"
				(at 38.1 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Mini-Circuits"
				(at 38.1 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 38.1 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, TRANSFORMER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Trans_TCM2-722X+_1_1"
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "2")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "IN")
					(number "3")
				)
				(pin passive line
					(at 30.48 -2.54 180)
					(length 2.54)
					(name "OUT_2")
					(number "4")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 2.54)
					(name "OUT_1")
					(number "5")
				)
				(pin no_connect line
					(at 26.67 -1.27 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
)
