(footprint "XFMR_ALSTOM_FIELDTR"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "FIELDTR Transformer - Body 17X17mm")
	(property "Reference" "REF**"
		(at 0 -9.30001 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_ALSTOM_FIELDTR"
		(at 0 9.30001 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "7"
		(at 4.15668 -5.82751 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "3"
		(at 2.11668 5.6225 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "2"
		(at -5.33591 -1.91009 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "6"
		(at -2.77128 -4.26546 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "5"
		(at 4.65668 3.0825 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "8"
		(at -4.90668 7.07251 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "3"
		(at 2.11668 5.6225 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "2"
		(at -5.33591 -1.91009 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "8"
		(at -4.90668 7.07251 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "6"
		(at -2.77128 -4.26546 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "7"
		(at 4.15668 -5.82751 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "5"
		(at 4.65668 3.0825 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "2" thru_hole circle
		(at -6.35 -3.81 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at 3.81 6.35 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at 6.35 3.81 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6" thru_hole circle
		(at -3.81 -6.35 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "7" thru_hole circle
		(at 6.35 -6.35 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "8" thru_hole circle
		(at -6.35 6.35 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
