(footprint "XFMR_CERN_HCRAASE001"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "CERN HF Power Transformer RM6")
	(property "Reference" "REF**"
		(at 0 -8.271 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_CERN_HCRAASE001"
		(at 0 8.271 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "6"
		(at 7.425 -0.9275 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -7.875 8.2975 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "2"
		(at -8.025 2.1225 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "5"
		(at 3.425 -7.4525 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "3"
		(at -1.9 8.3475 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "4"
		(at 7.375 -7.4525 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "2"
		(at -8.025 2.1225 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "4"
		(at 7.375 -7.4525 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "6"
		(at 7.425 -0.9275 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "1"
		(at -7.875 8.2975 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "5"
		(at 3.425 -7.4525 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "3"
		(at -1.9 8.3475 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at -6.35 6.35)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at -6.35 3.81)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at -3.81 6.375)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at 6.35 -6.35)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at 3.81 -6.35)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6" thru_hole circle
		(at 6.35 -3.81)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "7" thru_hole circle
		(at 6.35 6.35)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "8" thru_hole circle
		(at -6.35 -6.35)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
