(footprint "XFMR_CERN_HCRAJJU001"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "CERN HF Current transformer")
	(property "Reference" "REF**"
		(at 0 -10.75001 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_CERN_HCRAJJU001"
		(at 0 10.75001 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_poly
		(pts
			(xy -5.5 9.00001) (xy -5.5 -9.00001) (xy -5.5 -9.0985) (xy -5.46157 -9.29169) (xy -5.38619 -9.47368) (xy -5.27675 -9.63747) (xy -5.13747 -9.77676) (xy -4.97368 -9.88619) (xy -4.79169 -9.96158) (xy -4.5985 -10.00001) (xy -4.5 -10.00001) (xy 4.5 -10.00001) (xy 4.5985 -10.00001) (xy 4.79169 -9.96158) (xy 4.97368 -9.88619) (xy 5.13747 -9.77676) (xy 5.27675 -9.63747) (xy 5.38619 -9.47368) (xy 5.46157 -9.29169) (xy 5.5 -9.0985) (xy 5.5 -9.00001) (xy 5.5 9.00001) (xy 5.5 9.0985) (xy 5.46157 9.29169) (xy 5.38619 9.47368) (xy 5.27675 9.63747) (xy 5.13747 9.77676) (xy 4.97368 9.88619) (xy 4.79169 9.96158) (xy 4.5985 10) (xy 4.5 10.00001) (xy -4.5 10.00001) (xy -4.5985 10.00001) (xy -4.79169 9.96158) (xy -4.97368 9.88619) (xy -5.13747 9.77676) (xy -5.27675 9.63747) (xy -5.38619 9.47368) (xy -5.46157 9.29169) (xy -5.5 9.0985)
		)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_text user "11"
		(at 0.79743 -5.08682 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "20"
		(at -2.08682 2.79065 90)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "r1"
		(at 1.89159 8.13679 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -10.1 0)
		(size 8 8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.1)
		(solder_paste_margin -4)
	)
	(pad "2" smd rect
		(at 10.1 0)
		(size 8 8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.1)
		(solder_paste_margin -4)
	)
	(embedded_fonts no)
)
