(footprint "XFMR_CERN_HCRALWW"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "CERN HF Power Transformer RM8")
	(property "Reference" "REF**"
		(at -0.04057 -11.32325 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_CERN_HCRALWW"
		(at -0.04057 11.31161 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "7"
		(at 5.3975 -10.6725 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "2"
		(at -2.54 11.5525 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "12"
		(at -12.3825 6.4725 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "11"
		(at -11.43 2.6625 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "8"
		(at 1.5875 -10.355 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "5"
		(at 10.16 -1.1475 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -5.715 11.87 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "6"
		(at 10.795 -4.9575 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -5.715 11.87 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "7"
		(at 5.3975 -10.6725 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "5"
		(at 10.16 -1.1475 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "6"
		(at 10.795 -4.9575 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "2"
		(at -2.54 11.5525 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "11"
		(at -11.43 2.6625 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "8"
		(at 1.5875 -10.355 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "12"
		(at -12.3825 6.4725 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at -6.35 8.89 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at -3.81 8.89 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at 8.89 -3.81 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6" thru_hole circle
		(at 8.89 -6.35 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "7" thru_hole circle
		(at 6.35 -8.89 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "8" thru_hole circle
		(at 3.81 -8.89 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "11" thru_hole circle
		(at -8.89 3.81 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "12" thru_hole circle
		(at -8.89 6.35 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "13" thru_hole circle
		(at 8.89 8.89 180)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "14" thru_hole circle
		(at -8.89 -8.89 180)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
