(footprint "XFMR_CERN_HCRANDA002"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "CERN HF Power Transformer RM6")
	(property "Reference" "REF**"
		(at 1.93769 -15.5525 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_CERN_HCRANDA002"
		(at 1.93769 8.15391 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "5"
		(at 3.43329 -7.46646 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -7.875 8.2975 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "6"
		(at 7.88888 -3.18588 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "6"
		(at 8.46013 -11.5775 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "4"
		(at 7.95 -5.6775 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "2"
		(at -8.025 2.1225 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "3"
		(at -1.9 8.3475 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "4"
		(at 6.4 -11.5775 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "5"
		(at 4.25 -11.5775 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "2"
		(at -8.025 2.1225 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "5"
		(at 4.25 -11.5775 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "3"
		(at -1.9 8.3475 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "1"
		(at -7.875 8.2975 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "5"
		(at 3.43329 -7.46646 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "4"
		(at 7.95 -5.6775 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "6"
		(at 8.46013 -11.5775 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "6"
		(at 7.88888 -3.18588 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "4"
		(at 6.4 -11.5775 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at -6.36404 6.36396)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at -6.36404 3.81838)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at -3.81846 6.36396)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at 7.82679 -14.0525)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4-NC" thru_hole circle
		(at 6.36388 -6.36396)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at 5.12429 -14.0525)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5-NC" thru_hole circle
		(at 3.8183 -6.36396)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6" thru_hole circle
		(at 10.52929 -14.0525)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6-NC" thru_hole circle
		(at 6.36388 -3.81838)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "7" thru_hole circle
		(at 6.36388 6.36396)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "8" thru_hole circle
		(at -6.36404 -6.36396)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
