(footprint "XFMR_CERN_HCRANDA003"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "CERN HF Power Transformer RM6")
	(property "Reference" "REF**"
		(at 1.409675 -10.76484 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_CERN_HCRANDA003"
		(at 1.409675 10.76516 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "7"
		(at 13.88326 7.88039 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "12"
		(at 14.249845 -7.80961 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -10.63098 -7.80961 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "6"
		(at -10.740545 7.88039 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(pad "1" thru_hole oval
		(at -7.80016 -7.84484 180)
		(size 2.2 2)
		(drill 1.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at -7.80016 -5.65484 180)
		(size 2.2 2)
		(drill 1.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at -7.80016 -3.46484 180)
		(size 2.2 2)
		(drill 1.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at -7.80016 3.46516 180)
		(size 2.2 2)
		(drill 1.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at -7.80016 5.65516 180)
		(size 2.2 2)
		(drill 1.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at -7.80016 7.84516 180)
		(size 2.2 2)
		(drill 1.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole oval
		(at 10.61984 7.84516 180)
		(size 2.2 2)
		(drill 1.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole oval
		(at 10.61984 5.65516 180)
		(size 2.2 2)
		(drill 1.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole oval
		(at 10.61984 3.46516 180)
		(size 2.2 2)
		(drill 1.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole oval
		(at 10.61984 -3.46484 180)
		(size 2.2 2)
		(drill 1.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole oval
		(at 10.61984 -5.65484 180)
		(size 2.2 2)
		(drill 1.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole oval
		(at 10.61984 -7.84484 180)
		(size 2.2 2)
		(drill 1.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "MECH1" thru_hole circle
		(at -0.00016 -9.01484 180)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "MECH2" thru_hole circle
		(at -0.00016 9.01516 180)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
