(footprint "XFMR_CERN_HCRANQS"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "R2E-DCDC ACF Power Transformer [48V; 12V]")
	(property "Reference" "REF**"
		(at 0 -14.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_CERN_HCRANQS"
		(at 0 14.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "1"
		(at -13.7 -10.9775 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "7"
		(at 13.4 12.8225 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "12"
		(at 12.7 -11.4775 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "6"
		(at -13.7 12.1225 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "10"
		(at 8.41 -1.9175 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "3"
		(at -9.06 -1.9175 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "4"
		(at -9.06 3.1625 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "11"
		(at 8.51 -5.7275 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "9"
		(at 8.66 3.1625 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "8"
		(at 8.66 6.9725 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "5"
		(at -9.06 6.9725 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "7"
		(at 8.66 10.7825 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "12"
		(at 8.41 -9.5375 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "2"
		(at -9.06 -5.7275 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "6"
		(at -9.06 10.7825 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "1"
		(at -9.06 -9.5375 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(pad "1" thru_hole circle
		(at -10.16 -10.16 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at -10.16 -6.35 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at -10.16 -2.54 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at -10.16 2.54 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at -10.16 6.35 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6" thru_hole circle
		(at -10.16 10.16 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "7" thru_hole circle
		(at 10.16 10.16 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "8" thru_hole circle
		(at 10.16 6.35 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "9" thru_hole circle
		(at 10.16 2.54 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "10" thru_hole circle
		(at 10.16 -2.54 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "11" thru_hole circle
		(at 10.16 -6.35 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "12" thru_hole circle
		(at 10.16 -10.16 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "13" thru_hole circle
		(at 0 -12.7 180)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "14" thru_hole circle
		(at 0 12.7 180)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
