(footprint "XFMR_COILCRAFT_CS2106L"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "50/60 Hz Current Sense Transformer - Body 26.67X21.59mm")
	(property "Reference" "REF**"
		(at 0 -11.595 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_COILCRAFT_CS2106L"
		(at 0 11.595 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "1"
		(at -8.6 -5.6875 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "8"
		(at 8 -6.8775 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "3"
		(at -8.6 3.2025 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "5"
		(at 8 8.3625 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "2"
		(at -8.6 -1.8775 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "4"
		(at -8.6 8.2825 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "4"
		(at -8.6 8.2825 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "5"
		(at 8 8.3625 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "3"
		(at -8.6 3.2025 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "2"
		(at -8.6 -1.8775 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "8"
		(at 8 -6.8775 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "1"
		(at -8.6 -5.6875 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at -6.505 -6.35 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at -6.505 -2.54 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at -6.505 2.54 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at -6.505 7.62 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at 6.505 7.62 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "8" thru_hole circle
		(at 6.505 -7.62 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
