(footprint "XFMR_COMATEC_12052912"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "230VAC to 9.5VAC 2VA, Custom Transformer, Body 28mm x 33mm")
	(property "Reference" "REF**"
		(at 0 -17.30001 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_COMATEC_12052912"
		(at 0 17.30001 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "S1"
		(at 12.97198 0.85001 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "P1"
		(at -11.35302 0.87499 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "S1"
		(at 12.97198 0.85001 90)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "P1"
		(at -11.35302 0.87499 90)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at -10.00001 -10.00001)
		(size 2.3 2.3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at -10.00001 10.00001)
		(size 2.3 2.3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at 10.00001 -5)
		(size 2.3 2.3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at 10.00001 5)
		(size 2.3 2.3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
